1、 附件
采购清单
	编号
	货物名称
	技术参数
	数量
	质保期
	交货期
	备注

	1
	909线性灯玻璃
	见技术参数清单
	1000件
	两年
	20天
	


技术参数：采购物品是为配合高架线性灯维修使用，灯具具体参数如下。投标单位必须对工程现状预先勘察，对所投材料的安装条件充分了解。所投标材料必须能够满足现场安装条件。
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Jt¥{E8  Optics Performance

St # i Beam Angle 76° x 105°
Biok#iZk  Photometric Curve *HR

2 4t %  Reflector FAliE
JtWSH  Lamp Specification

d  f#  Brand GE

% B Type TS5 HeHAT
4T3k%%  Lampholder G5

3 % PowerSupply 28W
i Temperature 2700k/3000k/4000k/6500k
St i #  Luminous flux 26001m
SEIEH Color Rendering 85
F¥% @ Average life 20000Hrs
B %% IP&Class

BiKBi22% %%  Ingress Protection 1P65

(B g%  Safety Classification
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/=M Physical Performance
AT RIS
AT R
YR Reflector Material

Fixture Color
Fixture Material

R, AT PR AR
i

B 0.4mm PRELE, 4E
J£99.85%, A 4t ISR

WitHkE  Cover Material 3mm 3B A
BEHERE  Control Gear

& f#  Brand TRIDONIC/HEP

% 5 Type T B, i i AR PR
TyAH Power Factor: 098

# JE  Voitage 220-240V

B % Frequency 50/60Hz

%#RE  Installation position ITRA





[image: image3.png]feiafkle  Power Supply

fEH R  Voltage of power supply 220~240V
fHii#  Frequency of power supply 50/60Hz
EOEMHE  Accessory B2





